Input filter and fuses N1407		(400) 	1/1 

	Symbol	Description			Manufact.

C401 	Capacitor, polyester 	2.2uF +/-10% 	100V	Siemens 	BJ2512-E1225-K 
C402 	Capacitor, polyester 	2.2uF +/-1O% 	100V	Siemens 	B32512-E1225-K 
C403 	Capacitor, polyester 	2.2uF +/-10% 	100V	Siemens 	B32512-E1225-K 
C404 	Capacitor, polyester 	2.2uF +/-10% 	100V	Siemens 	B32512-E1225-K 
C405 	Capacitor, polyester 	2.2uF +/-10% 	l00V	Siemens 	B32512-E1225-K 
C406 	Capacitor, polyester 	2.2uF +/-10% 	100V	Siemens 	B32512-E1225-K 
C407 	Capacitor, polyester 	  1uF +/-20% 	100V	ERO 	MKT 1822-510-016 
C408 	Capacitor, polyester 	  1uF +/-20% 	100V	ERO 	MKT 1822-510-016 
C409 	Capacitor, electrolytic 	2200uF -10/+50%  40V	ROE 	EG 00 MG 422G 
C410 	Capacitor, electrolytic 	2200uF -10/+50%  40V	ROE 	EG 00 MG 422G 

D40l 	Diode 			Motorola 	MR750 
D402 	Diode 			Motorola 	MR750 

F401 	Fuse	10A Little fuse 			311010 
F402 	Fuse	35A Little fuse 			311035 

L401 	Coil 				S.P. TL354